|  |
| --- |
| **1 track sensor, robot production necessary** |
| **The use of infrared light detection,**  **anti-interference ability** |
| **The sensor adopts CTRT5000, which has high**  **sensitivity and stable performance** |
|  |
| **Operating voltage 5V, black line output low, white line output high level** |