315M super regeneration high frequency receiving module, wireless transmitting module, burglar alarm transmitter + receiver

|  |  |
| --- | --- |
| Product information | |
| kindly reminder | \* The VCC voltage should be consistent with the module operating voltage, and the power filter must be made;  \* The antenna has a great influence on the receiving effect of the module. It is better to connect the antenna with 1/4 wavelength, and generally use 50 ohm single core wire, the length of antenna is about 17cm 433M;  \* The position of the antenna also has influence on the effect of receiving module, antenna installation, as far as possible straight away from the shield, high pressure, and local interference; receiving frequency, decoding and oscillation resistance should use and emission matching;  \* No antenna, please bring your own antenna. |
| product description | Receive module technical parameter  working voltage：DC5V  Quiescent current：4MA  Receiving frequency：315MHZ  Receiving sensitivity：－105DB  Size：30\*14\*7mm  External antenna: 32CM single core wire, twisted into a spiral  Emitter technical parameters  Firing distance: 20-200 meters (voltage difference, effect is different)  Working voltage: 3.5-12V  Overall size：19\*19mm  Working mode：AM  transmission speed：4KB/S  Transmitted power：10mW  Emission frequency：315M  External antenna: 25cm common multi core or single core wire  The pins are arranged from left to right：（DATA；VCC；GND）  application environment  Remote control switch, receiving module, motorcycle, automobile anti-theft products, household products, anti-theft doors, electric shutter doors, windows, remote control socket, remote control LED, remote control, remote control audio electric door, garage door remote control, remote control, remote control gate gate, sliding door, remote control door opener, closed door control system, remote control curtain machine alarm host, alarm, remote control, remote control, remote control MP3 electric motorcycle etc.. |
|  |  |

